[2024-04-16 01:29:13:738:738025  COM18]:XIAOMI SOURCE TOOL EDL 2024
[2024-04-16 01:29:13:799:799356  COM18]:vboytest index:18
[2024-04-16 01:29:13:846:846224  COM18]:flash in thread name:COM18,id:17
[2024-04-16 01:29:13:908:908725  COM18]:sw in images
[2024-04-16 01:29:13:971:971221  COM18]:vboytest do open :
[2024-04-16 01:29:14:018:018101  COM18]: serial port COM18 opend successfully
[2024-04-16 01:29:14:064:064970  COM18]:[COM18]:start flash.
[2024-04-16 01:29:14:111:111846  COM18]:received hello packet
[2024-04-16 01:29:14:158:158743  COM18]:programmertype: 0
[2024-04-16 01:29:14:205:205597  COM18]:swPath:G:\Firmware Sementara\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global_2b7cfb215b\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global\images
[2024-04-16 01:29:14:221:221216  COM18]:download programmer file: G:\Firmware Sementara\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global_2b7cfb215b\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global\images\prog_firehose_ddr.elf
[2024-04-16 01:29:14:221:221216  COM18]:download programmer G:\Firmware Sementara\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global_2b7cfb215b\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global\images\prog_firehose_ddr.elf
[2024-04-16 01:29:27:014:014009  COM18]:Send done packet
[2024-04-16 01:29:27:014:014009  COM18]:file G:\Firmware Sementara\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global_2b7cfb215b\citrus_id_global_images_V14.0.2.0.SJFIDXM_20230425.0000.00_12.0_global\images\prog_firehose_ddr.elf transferred successfully
[2024-04-16 01:29:29:032:032997  COM18]:send nop command
[2024-04-16 01:29:29:032:032997  COM18]:send command:<?xml version="1.0" ?><data><nop verbose="0"  value="ping"/></data>
[2024-04-16 01:29:29:032:032997  COM18]:get response from target
[2024-04-16 01:29:29:048:048597  COM18]:resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: ufs: SAMSUNG" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Binary build date: Apr 13 2023 @ 21:00:36" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Binary build date: Apr 13 2023 @ 21:00:36
" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Chip serial num: 2402967633 (0x8f3a6051)" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Supported Functions (15):" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: program" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: read" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: nop" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: patch" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: configure" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: setbootablestoragedrive" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: erase" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: power" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: firmwarewrite" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: getstorageinfo" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: benchmark" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: emmc" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: ufs" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: fixgpt" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: getsha256digest" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: End of supported functions 15" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Calling handler for nop" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Binary build date: Apr 13 2023 @ 21:00:36
" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Chip serial num: 2402967633 (0x8f3a6051)" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: Supported Functions (15):" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: program" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: read" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: nop" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: patch" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: configure" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: setbootablestoragedrive" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: erase" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: power" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: firmwarewrite" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: getstorageinfo" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: benchmark" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: emmc" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: ufs" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: fixgpt" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: getsha256digest" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="INFO: End of supported functions 15" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="ACK" rawmode="false" /></data>


[2024-04-16 01:29:29:048:048597  COM18]:Chip serial num: INFO: Chip serial num: 2402967633 (0x8f3a6051)
[2024-04-16 01:29:29:111:111121  COM18]:send configure command
[2024-04-16 01:29:29:111:111121  COM18]:send command:<?xml version="1.0" ?><data><configure verbose="0" AlwaysValidate="0"  ZlpAwareHost="1"  MaxPayloadSizeToTargetInBytes="1048576" MemoryName="ufs" SkipStorageInit="0"/></data>
[2024-04-16 01:29:29:111:111121  COM18]:get response from target
[2024-04-16 01:29:29:126:126718  COM18]:resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[2024-04-16 01:29:29:876:876724  COM18]:no Binary dump
[2024-04-16 01:29:30:642:642383  COM18]:no Binary dump
[2024-04-16 01:29:31:386:386951  COM18]:no Binary dump
[2024-04-16 01:29:32:136:136905  COM18]:no Binary dump
[2024-04-16 01:29:32:199:199474  COM18]:edl authentication
[2024-04-16 01:29:32:199:199474  COM18]:authentication edl.
[2024-04-16 01:29:32:199:199474  COM18]:send command:<?xml version="1.0" ?><data> <sig TargetName="req" verbose="1"/></data>
[2024-04-16 01:29:32:199:199474  COM18]:get response from target
[2024-04-16 01:29:32:199:199474  COM18]:resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<sig TargetName="blob" value="AQAAALwBAABRYDqPMjHIUEdLWdS_R6KbqW_otQ" /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="ACK" rawmode="false" /></data>


[2024-04-16 01:29:32:277:277577  COM18]:origin:AQAAALwBAABRYDqPMjHIUEdLWdS_R6KbqW_otQ
[2024-04-16 01:29:32:277:277577  COM18]:SignEdl
[2024-04-16 01:31:16:955:955275  COM18]:System.IO.FileNotFoundException: Could not find file 'H:\DATA PHOENIX\AUTH_RIFAL\计算BLOB\HASIL EXTRACT\xst.sig'.
File name: 'H:\DATA PHOENIX\AUTH_RIFAL\计算BLOB\HASIL EXTRACT\xst.sig'
   at System.IO.__Error.WinIOError(Int32 errorCode, String maybeFullPath)
   at System.IO.FileStream.Init(String path, FileMode mode, FileAccess access, Int32 rights, Boolean useRights, FileShare share, Int32 bufferSize, FileOptions options, SECURITY_ATTRIBUTES secAttrs, String msgPath, Boolean bFromProxy, Boolean useLongPath, Boolean checkHost)
   at System.IO.FileStream..ctor(String path, FileMode mode, FileAccess access, FileShare share, Int32 bufferSize, FileOptions options, String msgPath, Boolean bFromProxy, Boolean useLongPath, Boolean checkHost)
   at System.IO.StreamReader..ctor(String path, Encoding encoding, Boolean detectEncodingFromByteOrderMarks, Int32 bufferSize, Boolean checkHost)
   at System.IO.File.InternalReadAllText(String path, Encoding encoding, Boolean checkHost)
   at System.IO.File.ReadAllText(String path)
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at System.IO.__Error.WinIOError(Int32 errorCode, String maybeFullPath)
   at System.IO.FileStream.Init(String path, FileMode mode, FileAccess access, Int32 rights, Boolean useRights, FileShare share, Int32 bufferSize, FileOptions options, SECURITY_ATTRIBUTES secAttrs, String msgPath, Boolean bFromProxy, Boolean useLongPath, Boolean checkHost)
   at System.IO.FileStream..ctor(String path, FileMode mode, FileAccess access, FileShare share, Int32 bufferSize, FileOptions options, String msgPath, Boolean bFromProxy, Boolean useLongPath, Boolean checkHost)
   at System.IO.StreamReader..ctor(String path, Encoding encoding, Boolean detectEncodingFromByteOrderMarks, Int32 bufferSize, Boolean checkHost)
   at System.IO.File.InternalReadAllText(String path, Encoding encoding, Boolean checkHost)
   at System.IO.File.ReadAllText(String path)
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
